{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["Removal","Installs","Exchange","Ofmats","Add ons"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Removal","index":0,"n_rows":40,"n_cols":10,"rows_kept":40,"merged":[[0,2,0,3],[0,5,0,6],[0,8,0,9],[1,0,19,0],[1,1,10,1],[11,1,19,1],[21,0,27,0],[21,1,27,1],[29,0,39,0],[29,1,32,1],[33,1,35,1],[36,1,39,1]],"flags":["formulas_cached_only"]}
[null,null,"STANDARD DIAPHRAGM METERS",null,null,"ROTARY METERS",null,null,"TURBINE METERS"]
["Adversarial Removal","LP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a low pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a low pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a low pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework"]
[null,null,"Contract sum (excluding V.A.T.): ","£…. plus purging on time and materials basis",null,"Special Features/Terms/Conditions:","This quotation is based on a low pressure service tier. If the pressure tier if found not to be low pressure, this will be subject to a new quotation or variation and planned meter works will not commence. ",null,"Special Features/Terms/Conditions:","This quotation is based on a low pressure service tier. If the pressure tier if found not to be low pressure, this will be subject to a new quotation or variation and planned meter works will not commence. "]
[null,null,"Analysis of Costs (all costs exclude V.A.T.) ","Purging:                     £ Purging on time and materials basis",null,"Analysis of Costs (all costs exclude V.A.T.) ","Lifting Gear, if required:                     £ 400 per day ",null,"Analysis of Costs (all costs exclude V.A.T.) ","Lifting Gear, if required:                     £ 400 per day "]
[null,null,"Contract sum (within the Quotation acceptance form ","£…. plus purging on time and materials basis",null,"Contract sum (with cost)","…, (excluding lifting gear changes)",null,"Contract sum (with cost)","…, (excluding lifting gear changes)"]
[null,null,"Special Features/Terms/Conditions:","This quotation is based on a low pressure service tier. If the pressure tier if found not to be low pressure, this will be subject to a new quotation or variation and planned meter works will not commence. ",null,"Contract sum (no cost)","…., (including lifting gear charges)",null,"Contract sum (no cost)","…., (including lifting gear charges)"]
[{"$nulls":5},"Special Features/Terms/Conditions:","Lifting gear if required will be charged at a rate of £400 per day",null,"Special Features/Terms/Conditions:","Lifting gear if required will be charged at a rate of £400 per day"]
[{"$nulls":5},"Contract sum (excluding V.A.T.): ","£…. plus purging on time and materials basis",null,"Contract sum (excluding V.A.T.): ","£…. plus purging on time and materials basis"]
[{"$nulls":5},"Analysis of Costs (all costs exclude V.A.T.) ","Purging:                     £ Purging on time and materials basis",null,"Analysis of Costs (all costs exclude V.A.T.) ","Purging:                     £ Purging on time and materials basis"]
[{"$nulls":5},"Contract sum (within the Quotation acceptance form ","£…. plus purging on time and materials basis",null,"Contract sum (within the Quotation acceptance form ","£…. plus purging on time and materials basis"]
[null,"MP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a medium pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a medium pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a medium pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework"]
[null,null,"Contract sum (excluding V.A.T.): ","£…. plus purging on time and materials basis",null,"Analysis of Costs (all costs exclude V.A.T.) ","Lifting Gear, if required:                     £ 400 per day ",null,"Analysis of Costs (all costs exclude V.A.T.) ","Lifting Gear, if required:                     £ 400 per day "]
[null,null,"Analysis of Costs (all costs exclude V.A.T.) ","Purging:                     £ Purging on time and materials basis",null,"Contract sum (with cost)","…, (excluding lifting gear changes)",null,"Contract sum (with cost)","…, (excluding lifting gear changes)"]
[null,null,"Contract sum (within the Quotation acceptance form ","£…. plus purging on time and materials basis",null,"Contract sum (no cost)","…., (including lifting gear charges)",null,"Contract sum (no cost)","…., (including lifting gear charges)"]
[{"$nulls":5},"Special Features/Terms/Conditions:","Lifting gear if required will be charged at a rate of £400 per day",null,"Special Features/Terms/Conditions:","Lifting gear if required will be charged at a rate of £400 per day"]
[{"$nulls":5},"Contract sum (excluding V.A.T.): ","£…. plus purging on time and materials basis",null,"Contract sum (excluding V.A.T.): ","£…. plus purging on time and materials basis"]
[{"$nulls":5},"Analysis of Costs (all costs exclude V.A.T.) ","Purging:                     £ Purging on time and materials basis",null,"Analysis of Costs (all costs exclude V.A.T.) ","Purging:                     £ Purging on time and materials basis"]
[{"$nulls":5},"Contract sum (within the Quotation acceptance form ","£…. plus purging on time and materials basis",null,"Contract sum (within the Quotation acceptance form ","£…. plus purging on time and materials basis"]
[]
["Standard Removal","LP","Section within letter","Standard wording"]
[null,null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a low pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework"]
[null,null,"Contract sum (excluding V.A.T.): ","£…. plus purging on time and materials basis"]
[null,null,"Analysis of Costs (all costs exclude V.A.T.) ","Purging:                     £ Purging on time and materials basis"]
[null,null,"Contract sum (within the Quotation acceptance form ","£…. plus purging on time and materials basis"]
[null,null,"Special Features/Terms/Conditions:","This quotation is based on a low pressure service tier. If the pressure tier if found not to be low pressure, this will be subject to a new quotation or variation and planned meter works will not commence. "]
[null,null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. "]
[]
["Removal","LP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a low pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a low pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a low pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework"]
[null,null,"Special Features/Terms/Conditions:","This quotation is based on a low pressure service tier. If the pressure tier if found not to be low pressure, this will be subject to a new quotation or variation and planned meter works will not commence. ",null,"Special Features/Terms/Conditions:","This quotation is based on a low pressure service tier. If the pressure tier if found not to be low pressure, this will be subject to a new quotation or variation and planned meter works will not commence. ",null,"Special Features/Terms/Conditions:","This quotation is based on a low pressure service tier. If the pressure tier if found not to be low pressure, this will be subject to a new quotation or variation and planned meter works will not commence. "]
[null,null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. ",null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. ",null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. "]
[null,"MP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a medium pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a medium pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a medium pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework"]
[null,null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. ",null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. ",null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. "]
[null,"IP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Analysis of Costs (all costs exclude V.A.T.) ","IGE/GL/5 Design Appraisal :               £484",null,"Analysis of Costs (all costs exclude V.A.T.) ","IGE/GL/5 Design Appraisal :               £484",null,"Analysis of Costs (all costs exclude V.A.T.) ","IGE/GL/5 Design Appraisal :               £484"]
[null,null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a intermediate pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a intermediate pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework",null,"Full Description of Works to be Carried Out by National Grid Metering","Removal of a intermediate pressure xxx (insert meter model) diaphragm meter module MSN xxxxx (insert serial number) and purging of downstream pipework"]
[null,null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. ",null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. ",null,"Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. "]

{"sheet":"Installs","index":1,"n_rows":17,"n_cols":10,"rows_kept":17,"merged":[[0,2,0,3],[0,5,0,6],[0,8,0,9],[1,0,16,0],[1,1,8,1],[9,1,16,1]],"flags":["formulas_cached_only"]}
[null,null,"STANDARD DIAPHRAGM METERS",null,null,"ROTARY METERS",null,null,"TURBINE METERS"]
["Standard Installation","LP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order.",null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order.",null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order."]
[null,null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed"]
[null,null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed"]
[null,null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 25 mbar under Qmax load at the ECV outlet point",null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 25 mbar under Qmax load at the ECV outlet point",null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 25 mbar under Qmax load at the ECV outlet point"]
[null,null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily.",null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily.",null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily."]
[null,null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place.",null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place.",null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place."]
[null,null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh.",null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh.",null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh."]
[null,"MP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order.",null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order.",null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order."]
[null,null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed"]
[null,null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed"]
[null,null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of nnn (insert design minimum pressure) mbar under Qmax load at the ECV outlet point",null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of nnn (insert design minimum pressure) mbar under Qmax load at the ECV outlet point",null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of nnn (insert design minimum pressure) mbar under Qmax load at the ECV outlet point"]
[null,null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module offered is a xxxx (twin/single) stream supply with only a nominal bypass facility.  The bypass is only used during maintenance, and is only sized to maintain gas pressure downstream. Please note that during maintenance it will be necessary to disrupt supplies. ",null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module offered is a xxxx (twin/single) stream supply with only a nominal bypass facility.  The bypass is only used during maintenance, and is only sized to maintain gas pressure downstream. Please note that during maintenance it will be necessary to disrupt supplies. ",null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module offered is a xxxx (twin/single) stream supply with only a nominal bypass facility.  The bypass is only used during maintenance, and is only sized to maintain gas pressure downstream. Please note that during maintenance it will be necessary to disrupt supplies. "]
[null,null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place.",null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place.",null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place."]
[null,null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh.",null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh.",null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh."]

{"sheet":"Exchange","index":2,"n_rows":23,"n_cols":10,"rows_kept":23,"merged":[[0,2,0,3],[0,5,0,6],[0,8,0,9],[1,0,19,0],[1,1,8,1],[12,1,22,1]],"flags":["formulas_cached_only"]}
[null,null,"STANDARD DIAPHRAGM METERS",null,null,"ROTARY METERS",null,null,"TURBINE METERS"]
["Standard Exchange","LP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order.",null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order.",null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order."]
[null,null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed"]
[null,null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed"]
[null,null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 25 mbar under Qmax load at the ECV outlet point",null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 25 mbar under Qmax load at the ECV outlet point",null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 25 mbar under Qmax load at the ECV outlet point"]
[null,null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily.",null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily.",null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily."]
[null,null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place.",null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place.",null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place."]
[null,null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh.",null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh.",null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh."]
[null,null,"Special Features/Terms/Conditions: ","This quotation is based on the exchange being completed on the same day and the new meter module being attached to the existing ECV.",null,"Special Features/Terms/Conditions: ","This quotation is based on the exchange being completed on the same day and the new meter module being attached to the existing ECV.",null,"Special Features/Terms/Conditions: ","This quotation is based on the exchange being completed on the same day and the new meter module being attached to the existing ECV."]
[null,null,"Special Features/Terms/Conditions ","Please note that this quotation is based on two visits, first visit for the removal and purging of the existing meter module and the second to install a new meter module after the service alteration.",null,"Special Features/Terms/Conditions ","Please note that this quotation is based on two visits, first visit for the removal and purging of the existing meter module and the second to install a new meter module after the service alteration.",null,"Special Features/Terms/Conditions ","Please note that this quotation is based on two visits, first visit for the removal and purging of the existing meter module and the second to install a new meter module after the service alteration."]
[null,null,"Description of Works to be Carried Out by 3rd Party","Any service alteration required will need to be actioned by the UIP. Any outlet pipework alterations and the outlet pipework connection to the meter module will need to be actioned by others.",null,"Description of Works to be Carried Out by 3rd Party","Any service alteration required will need to be actioned by the UIP. Any outlet pipework alterations and the outlet pipework connection to the meter module will need to be actioned by others.",null,"Description of Works to be Carried Out by 3rd Party","Any service alteration required will need to be actioned by the UIP. Any outlet pipework alterations and the outlet pipework connection to the meter module will need to be actioned by others."]
[null,"MP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order.",null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order.",null,"Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative and are based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order."]
[null,null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure to provide adequate housing will result in the job not being completed"]
[null,null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed",null,"Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: L nnn mm x W nnn mm x H nnn mm . Failure not to provide acurate base will result in the job not being completed"]
[null,null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of nnn (insert design minimum pressure) mbar under Qmax load at the ECV outlet point",null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of nnn (insert design minimum pressure) mbar under Qmax load at the ECV outlet point",null,"Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of nnn (insert design minimum pressure) mbar under Qmax load at the ECV outlet point"]
[null,null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module offered is a singlestream supply with only a nominal bypass facility.  The bypass is only used during maintenance, and is only sized to maintain gas pressure downstream. Please note that during maintenance it will be necessary to disrupt supplies. ",null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module offered is a single stream supply with only a nominal bypass facility.  The bypass is only used during maintenance, and is only sized to maintain gas pressure downstream. Please note that during maintenance it will be necessary to disrupt supplies. ",null,"Special Features/Terms/Conditions: ","This quotation is based on a xxxxxx (insert inlet orientation) inlet and xxxxxx (insert outlet orientation) outlet and the ECV being installed to the dimensions provided\n\nThe meter module offered is a single stream supply with only a nominal bypass facility.  The bypass is only used during maintenance, and is only sized to maintain gas pressure downstream. Please note that during maintenance it will be necessary to disrupt supplies. "]
[null,null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place.",null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place.",null,"Special Features/Terms/Conditions: ","It is critical that the module inlet dimensions and orientation are given to the UIP when service works are taken place."]
[null,null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh.",null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh.",null,"Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh."]
[null,null,"Special Features/Terms/Conditions: ","This quotation is based on the exchange being completed on the same day and the new meter module being attached to the existing ECV.",null,"Special Features/Terms/Conditions: ","This quotation is based on the exchange being completed on the same day and the new meter module being attached to the existing ECV.",null,"Special Features/Terms/Conditions: ","This quotation is based on the exchange being completed on the same day and the new meter module being attached to the existing ECV."]
[null,null,"Special Features/Terms/Conditions ","Please note that this quotation is based on two visits, first visit for the removal and purging of the existing meter module and the second to install a new meter module after the service alteration.",null,"Special Features/Terms/Conditions ","Please note that this quotation is based on two visits, first visit for the removal and purging of the existing meter module and the second to install a new meter module after the service alteration.",null,"Special Features/Terms/Conditions ","Please note that this quotation is based on two visits, first visit for the removal and purging of the existing meter module and the second to install a new meter module after the service alteration."]
[null,null,"Description of Works to be Carried Out by 3rd Party","Any service alteration required will need to be actioned by the UIP. Any outlet pipework alterations and the outlet pipework connection to the meter module will need to be actioned by others.",null,"Description of Works to be Carried Out by 3rd Party","Any service alteration required will need to be actioned by the UIP. Any outlet pipework alterations and the outlet pipework connection to the meter module will need to be actioned by others.",null,"Description of Works to be Carried Out by 3rd Party","Any service alteration required will need to be actioned by the UIP. Any outlet pipework alterations and the outlet pipework connection to the meter module will need to be actioned by others."]

{"sheet":"Ofmats","index":3,"n_rows":5,"n_cols":10,"rows_kept":5,"merged":[[0,2,0,3],[0,5,0,6],[0,8,0,9],[1,0,4,0],[1,1,2,1],[3,1,4,1]],"flags":["formulas_cached_only"]}
[null,null,"STANDARD DIAPHRAGM METERS",null,null,"ROTARY METERS",null,null,"TURBINE METERS"]
["Ofmats","LP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Special Features/Terms/Conditions:","This charge will only be applicable if the meter accuracy test identifies the meter to be working correctly. ",null,"Special Features/Terms/Conditions:","This charge will only be applicable if the meter accuracy test identifies the meter to be working correctly. ",null,"Special Features/Terms/Conditions:","This charge will only be applicable if the meter accuracy test identifies the meter to be working correctly. "]
[null,"MP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Special Features/Terms/Conditions:","This charge will only be applicable if the meter accuracy test identifies the meter to be working correctly. ",null,"Special Features/Terms/Conditions:","This charge will only be applicable if the meter accuracy test identifies the meter to be working correctly. ",null,"Special Features/Terms/Conditions:","This charge will only be applicable if the meter accuracy test identifies the meter to be working correctly. "]

{"sheet":"Add ons","index":4,"n_rows":9,"n_cols":10,"rows_kept":9,"merged":[[0,2,0,3],[0,5,0,6],[0,8,0,9],[1,0,8,0],[1,1,4,1],[5,1,8,1]],"flags":["formulas_cached_only"]}
[null,null,"STANDARD DIAPHRAGM METERS",null,null,"ROTARY METERS",null,null,"TURBINE METERS"]
["Add-Ons","LP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Special Features/Terms/Conditions: ","This quotation is based on there being a working LF connection on the existing meter",null,"Special Features/Terms/Conditions: ","This quotation is based on there being a working LF connection on the existing meter",null,"Special Features/Terms/Conditions: ","This quotation is based on there being a working LF connection on the existing meter"]
[null,null,"Special Features/Terms/Conditions: ","This quotation does not include for the provision of a separate instrumentation cabinet.",null,"Special Features/Terms/Conditions: ","This quotation does not include for the provision of a separate instrumentation cabinet.",null,"Special Features/Terms/Conditions: ","This quotation does not include for the provision of a separate instrumentation cabinet."]
[null,null,"Special Features/Terms/Conditions: ","Electrical Connections to gas meters are subject to the assessment of the hazardous area around the meter. This is largely affected by the ventilation in the housing. Should the ventilation be found to be inadequate the connection will not be made and the requirements to allow the connection reported to you. ",null,"Special Features/Terms/Conditions: ","Electrical Connections to gas meters are subject to the assessment of the hazardous area around the meter. This is largely affected by the ventilation in the housing. Should the ventilation be found to be inadequate the connection will not be made and the requirements to allow the connection reported to you. ",null,"Special Features/Terms/Conditions: ","Electrical Connections to gas meters are subject to the assessment of the hazardous area around the meter. This is largely affected by the ventilation in the housing. Should the ventilation be found to be inadequate the connection will not be made and the requirements to allow the connection reported to you. "]
[null,"MP","Section within letter","Standard wording",null,"Section within letter","Standard wording",null,"Section within letter","Standard wording"]
[null,null,"Special Features/Terms/Conditions: ","This quotation is based on there being a working LF connection on the existing meter",null,"Special Features/Terms/Conditions: ","This quotation is based on there being a working LF connection on the existing meter",null,"Special Features/Terms/Conditions: ","This quotation is based on there being a working LF connection on the existing meter"]
[null,null,"Special Features/Terms/Conditions: ","This quotation does not include for the provision of a separate instrumentation cabinet.",null,"Special Features/Terms/Conditions: ","This quotation does not include for the provision of a separate instrumentation cabinet.",null,"Special Features/Terms/Conditions: ","This quotation does not include for the provision of a separate instrumentation cabinet."]
[null,null,"Special Features/Terms/Conditions: ","Electrical Connections to gas meters are subject to the assessment of the hazardous area around the meter. This is largely affected by the ventilation in the housing. Should the ventilation be found to be inadequate the connection will not be made and the requirements to allow the connection reported to you. ",null,"Special Features/Terms/Conditions: ","Electrical Connections to gas meters are subject to the assessment of the hazardous area around the meter. This is largely affected by the ventilation in the housing. Should the ventilation be found to be inadequate the connection will not be made and the requirements to allow the connection reported to you. ",null,"Special Features/Terms/Conditions: ","Electrical Connections to gas meters are subject to the assessment of the hazardous area around the meter. This is largely affected by the ventilation in the housing. Should the ventilation be found to be inadequate the connection will not be made and the requirements to allow the connection reported to you. "]