{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Others","Removals - Reposition","Install - Exchange - OFMATs","Manufacturer Quotes ONLY"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Others","index":0,"n_rows":16,"n_cols":4,"rows_kept":16,"merged":[[1,0,1,3],[2,0,4,0],[5,0,5,3],[6,0,7,0],[8,0,8,3],[9,0,11,0],[12,0,12,3],[13,0,15,0]],"flags":["formulas_cached_only"]}
[null,"Scenario","Section Within Letter","Standard Wording"]
[]
["All Job Types","NON Supplier Quotes for all the jobs","Special Features/Terms/Conditions:","Payment of the contract sum plus VAT must be submitted with your Acceptance of this quotation if you wish National Grid Metering to proceed with this work request"]
[null,"Datalogger on SAP (install or exchange)","Special Features/Terms/Conditions:","This quote does not include the provision or maintenance of a Datalogger  "]
[null,"Datalogger on SAP (removal)","Special Features/Terms/Conditions:","This quote does not include the removal of the Datalogger. Please make the necessary arrangements with the Gas Transporter."]
[]
["Cancellations","Request for metering pressure greater than 21mb for an LP service","Special Features/Terms/Conditions","The Service Pressure to this site will not support the design criteria requested"]
[null,"The current meter is capable of suppling the requested Load","Special Features/Terms/Conditions","The Qmax specified in your quotation request is less than that of the meter currently installed at this Meter Point. \n\nIf the existing meter is capable of accurately registering the range of consumption required at the site it will be considered 'fit for purpose' and will therefore not be replaced. Where a meter is considered 'fit for purpose', but the customer can demonstrate that 2% of the annual gas load (AQ) flows through the meter at less than the meter's official Qmin, the meter could be considered for replacement and downsizing."]
[]
["EMS & AMR","EMS connection to existing meter","Special Features/Terms/Conditions: ","This quotation is based on there being a working LF connection on the existing meter"]
[null,"AMR with new meter","Special Features/Terms/Conditions: ","Please note the installation and connection of the AMR device is non chargeable and will be installed at a future date"]
[null,"All EMS connection requests\n(do not use if Housing has been requested in quotation)","Special Features/Terms/Conditions: ","Electrical Connections to gas meters are subject to the assessment of the hazardous area around the meter, this is largely affected by the ventilation in the housing, should the ventilation be found to be inadequate the connection will not be made and the requirements to allow the connection reported to you. This quotation does not include for the provision of a separate instrumentation cabinet."]
[]
["GT1","GT1 Passed","Special Features/Terms/Conditions: ","This Quotation is based on the Medium Pressure Tier of 270 mbar,"]
[null,"(GT1 Failures) Prior to Quoting","Special Features/Terms/Conditions: ","This Quotation is based on the Medium Pressure Tier of 270 mbar, however we believe the pressure tier to be XXX. Please verify the pressure tier with the Gas Transportor prior to acceptance."]
[null,"GT1 - where the GT1 has not returned","Special Features/Terms/Conditions: ","This quote is based on a medium pressure tier of 270 mbars and is only suitable for this pressure tier.  Please verify the pressure tier with the Gas Transporter prior to acceptance to confirm suitability of the design."]

{"sheet":"Removals - Reposition","index":1,"n_rows":23,"n_cols":4,"rows_kept":23,"merged":[[1,0,1,3],[2,0,12,0],[2,1,7,1],[4,2,5,2],[6,2,7,2],[14,0,16,0],[18,0,22,0],[18,1,19,1],[18,2,19,2]],"flags":["formulas_cached_only"]}
[null,"Scenario","Section Within Letter","Standard Wording"]
[]
["Removals","Adversarial & Non adversarial U16 to U40 ","Full Description of Works to be Carried Out by National Grid Metering","Removal and purge of (insert meter type), MSN (insert serial number) "]
[null,null,"Contract sum (excluding V.A.T.): ","£…. plus purging on time and materials basis"]
[null,null,"Analysis of Costs (all costs exclude V.A.T.) ","Purging:                     £ Purging on time and materials basis"]
[{"$nulls":3},"Lifting Gear, if required:                     £ 220.00 per day"]
[null,null,"Contract sum (within the Quotation acceptance form ","£…. plus purging on time and materials basis"]
[{"$nulls":3},"…, excluding lifting gear changes."]
[null,"Non adversarial U65 and above ","Full Description of Works to be Carried Out by National Grid Metering","Removal of (insert meter type), MSN (insert serial number) and purging of downstream pipework"]
[null,"Lifting Gear on Mip or Unknown meter (not including LP Diaphragms)","Special Features/Terms/Conditions:","Lifting gear if required will be charged at a rate of £220 per day"]
[null,"Purging costs not requested. ","Special Features/Terms/Conditions:","Where purging of downstream supplies is necessary but has not been requested as part of the meter removal work, the meter will not be removed until the downstream supplies have been made safe by purging. "]
[null,"Pressure tier unknown (caveat not required where Labour rate x man hours is used)","Special Features/Terms/Conditions:","This quotation is based on an inlet pressure of up to 75 mbar. If upon commencement of work the inlet pressure is found to be higher than 75 mbar, the planned meter works will not commence. "]
[null,"Purging costs requested but site survey results confirm no purging will be required","Special Features/Terms/Conditions:","Please note that following a visit to the site, it has been confirmed that no purging will be required as …"]
[]
["All Job Types","NON Supplier Quotes for all the jobs","Special Features/Terms/Conditions:","Payment of the contract sum plus VAT must be submitted with your Acceptance of this quotation if you wish National Grid Metering to proceed with this work request"]
[null,"Datalogger on SAP (install or exchange)","Special Features/Terms/Conditions:","This quote does not include the provision or maintenance of a Datalogger  "]
[null,"Datalogger on SAP (removal)","Special Features/Terms/Conditions:","This quote does not include the removal of the Datalogger. Please make the necessary arrangements with the Gas Transporter."]
[]
["Reposition","All jobs","Special Features/Terms/Conditions ","This quote is based on the new service being sized and positioned the same as the existing service in the new location."]
[{"$nulls":3},"Any service alteration required will need to be actioned by the UIP. Any outlet pipework alterations and the outlet pipework connection to the meter module will need to be actioned by others."]
[null,"Disconnection & Reconnection","Special Features/Terms/Conditions ","Please note that this quotation is based on two visits, first visit for the disconnection and the second to reconnect the same meter."]
[null,"  2 Visit Jobs ( Same meter)","Special Features/Terms/Conditions ","Please be aware that the meter will need to be stored in a secure location and free from any contamination. Further charges may be incurred if the meter is damaged."]
[null,"New Housing Requested","Special Features/Terms/Conditions ","Please note that the sizes and dimensions stated are indicative based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order.\n"]

{"sheet":"Install - Exchange - OFMATs","index":2,"n_rows":28,"n_cols":4,"rows_kept":28,"merged":[[1,0,1,3],[2,0,4,0],[5,0,5,3],[6,0,21,0],[11,1,12,1],[11,2,12,2],[13,1,14,1],[13,2,14,2],[20,1,21,1],[20,2,21,2],[22,0,22,3],[25,0,27,0]],"flags":["formulas_cached_only"]}
[null,"Scenario","Section Within Letter","Standard Wording"]
[]
["All Job Types","NON Supplier Quotes for all the jobs","Special Features/Terms/Conditions:","Payment of the contract sum plus VAT must be submitted with your Acceptance of this quotation if you wish National Grid Metering to proceed with this work request"]
[null,"Datalogger on SAP (install or exchange)","Special Features/Terms/Conditions:","This quote does not include the provision or maintenance of a Datalogger  "]
[null,"Datalogger on SAP (removal)","Special Features/Terms/Conditions:","This quote does not include the removal of the Datalogger. Please make the necessary arrangements with the Gas Transporter."]
[]
["Installations and Exchanges                                                                   Installations and Exchanges","No lifting gear charge available, not including low pressure diaphragm meters.","Special Features/Terms/Conditions: ","Lifting gear if required will be charged at a rate of £220 per day "]
[null,"All Jobs","Special Features/Terms/Conditions: ","Please note that all the sizes and dimensions stated are indicative based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order."]
[null,"Housing not requested","Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: nnn mm L x nnn mm W x nnn mm H."]
[null,"Base not requested","Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: nnn mm L x nnn mm W x nnn mm H."]
[null,"Site survey report indicates that there may be a problem with the service","Special Features/Terms/Conditions: ","The existing service may not be adequate for the proposed new meter.  You will need to confirm its suitability with the gas transporter prior to accepting this quotation."]
[null,"All LP Meter installation and exchange","Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 25 mbar under Qmax load at the ECV outlet point"]
[{"$nulls":3},"This quotation is based on a vertical inlet and outlet unless otherwise specified and the ECV being installed to industry standard.\n\nThe meter module is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily."]
[null,"All MP Meter installation and exchange","Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 270 mbar under Qmax load at the ECV outlet point"]
[{"$nulls":3},"This quotation is based on a vertical inlet and outlet unless otherwise specified and the ECV being installed to industry standard.\n\nThe meter module offered is a single stream supply with only a nominal bypass facility.  The bypass is only used during maintenance, and is only sized to maintain gas pressure downstream. Please note that during maintenance it will be necessary to disrupt supplies. "]
[null,"All MP jobs where the pressure tier isn't stated","Special Features/Terms/Conditions: ","This Quotation is based on the Medium Pressure Tier of 270mbar"]
[null,"Meter Installation with Booster","Special Features/Terms/Conditions: ","It will be necessary for the end-user to ensure that a non-return valve is installed upstream of any booster or compressor that may be installed to protect the meter installation from back pressure in the event of failure of the booster or compressor."]
[null,"Meter installation for a special site (hospital, prison, process load etc) where the request did not specify a twin-stream governor meter module","Special Features/Terms/Conditions: ","The meter module offered is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily. If the load that this meter will supply is critical we recommend that you request a twin-stream design with a full bypass sufficient to maintain supply at all times."]
[null,"Meter Exchange (LP & MP)","Special Features/Terms/Conditions: ","This quotation is based on the exchange being completed on the same day and the new meter module being attached to the existing Emergency Control Valve (ECV)"]
[null,"2 Visit Meter Exchange\n(LP & MP)","Special Features/Terms/Conditions ","Please note that this quotation is based on two visits, first visit for the removal and purging of the existing meter module and the second to install a new meter module after the service upgrade."]
[null,"All jobs","Special Features/Terms/Conditions: ","Please refer to the Technical Specifications sheets included within this quotation for details of this design"]
[{"$nulls":3},"The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh."]
[]
["OFMAT","All OFMAT Quotes","Special Features/Terms/Conditions:","This charge will only be applicable if the meter accuracy test identifies the meter to be working correctly."]
[]
["EMS & AMR","EMS connection to existing meter","Special Features/Terms/Conditions: ","This quotation is based on there being a working LF connection on the existing meter"]
[null,"AMR with new meter","Special Features/Terms/Conditions: ","Please note the installation and connection of the AMR device is non chargeable and will be installed at a future date"]
[null,"All EMS connection requests\n(do not use if Housing has been requested in quotation)","Special Features/Terms/Conditions: ","Electrical Connections to gas meters are subject to the assessment of the hazardous area around the meter, this is largely affected by the ventilation in the housing, should the ventilation be found to be inadequate the connection will not be made and the requirements to allow the connection reported to you. This quotation does not include for the provision of a separate instrumentation cabinet."]

{"sheet":"Manufacturer Quotes ONLY","index":3,"n_rows":51,"n_cols":6,"rows_kept":51,"merged":[[1,0,1,4],[2,0,4,0],[5,0,5,4],[6,0,10,0],[8,5,10,5],[11,0,11,4],[12,0,31,0],[13,1,14,1],[13,2,14,2],[21,1,22,1],[21,2,22,2],[21,3,22,3],[23,1,24,1],[23,2,24,2],[23,3,24,3],[32,0,32,4],[33,0,34,0],[35,0,35,4],[36,0,38,0],[39,0,39,4],[40,0,42,0],[43,0,43,4],[44,0,50,0]],"flags":["formulas_cached_only"]}
[null,"For","Scenario","Section Within Letter","Standard Wording"]
[]
["All Job Types","NON Supplier Quotes for all the jobs",null,"Special Features/Terms/Conditions:","Payment of the contract sum plus VAT must be submitted with your Acceptance of this quotation if you wish National Grid Metering to proceed with this work request"]
[null,"All jobs","Datalogger on SAP (install or exchange)","Special Features/Terms/Conditions:","This quote does not include the provision or maintenance of a Datalogger  "]
[null,"All Jobs","Datalogger on SAP (removal)","Special Features/Terms/Conditions:","This quote does not include the removal of the Datalogger. Please make the necessary arrangements with the Gas Transporter."]
[]
["Housing and Base","All Jobs","Housing not requested","Special Features/Terms/Conditions: ","Housings must have a free ventilation area equal to/exceeding 3% floor area. Minimum Housing requirements for this module are: nnn mm L x nnn mm W x nnn mm H."]
[null,"All Jobs","Base not requested","Special Features/Terms/Conditions: ","Minimum Base dimension requirements for this module are: nnn mm L x nnn mm W x nnn mm H."]
[null,"Actaris Designs","Where we are providing the Housing","Special Features/Terms/Conditions: ","The housing costs and dimensions provided are indicative; these must be confirmed at placement of order.","Do not used these yet.  Dafydd is still reviewing the caveat.  Pending George's meeting with Actaris."]
[null,"Actaris Designs","Where we are providing the Base","Special Features/Terms/Conditions: ","The base costs and dimensions provided are indicative; these must be confirmed at placement of order."]
[null,"Actaris Designs","Where we are providing the Housing and the Base","Special Features/Terms/Conditions: ","The housing and base costs and dimensions provided are indicative; these must be confirmed at placement of order."]
[]
["Installs and Exchanges                                                        Installs and Exchanges","All Jobs","Site survey report indicates that there may be a problem with the service","Special Features/Terms/Conditions: ","The existing service may not be adequate for the proposed new meter.  You will need to confirm its suitability with the gas transporter prior to accepting this quotation."]
[null,"All Jobs","Manufacturer has indicated a delivery time longer than the contact lead time","Page two\nIndicative Lead time from Acceptance to Physical Commencement","nnn working days. Please note that the manufacturer has indicated that it could take up to nnn working days to build and deliver the new meter module."]
[{"$nulls":3},"Special Features/Terms/Conditions: ","Please note that the manufacturer has indicated that it could take up to nnn working days to build and deliver the new meter module."]
[null,"All Jobs","Bespoke Meter installation","Full Description of Works to be Carried Out by National Grid Metering","Provide and install a xxx pressure xxx stream governor xxx meter module capable of passing nnn kWh of gas demand."]
[null,"All Jobs","All","Special Features/Terms/Conditions: ","Please note that the sizes and dimensions stated are indicative based on current practice at the time of quotation. These are subject to change and must be confirmed at placement of order."]
[null,"All Jobs","All","Special Features/Terms/Conditions: ","The proposed meter module has a Qmin of nnn kWh and is based on the requested Qmax of nnn kWh."]
[null,"MP Jobs","All MP jobs where the pressure tier isn't stated","Special Features/Terms/Conditions: ","This Quotation is based on the Medium Pressure Tier of 270mbar"]
[null,"LP Jobs","All LP Meter installation and exchange","Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 25 mbar under Qmax load at the ECV outlet point"]
[null,"MP Jobs","All MP Meter installation and exchange","Special Features/Terms/Conditions: ","The Supply Point must be suitably sized and positioned to provide a minimum pressure of 270 mbar under Qmax load at the EVC outlet point"]
[null,"LP Jobs","All","Special Features/Terms/Conditions: ","This quotation is based on a vertical inlet and a vertical outlet unless otherwise specified and the ECV being installed to the above dimensions."]
[{"$nulls":4},"The meter module is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily."]
[null,"MP Jobs","All","Special Features/Terms/Conditions: ","This quotation is based on a vertical inlet and a vertical outlet unless otherwise specified and the ECV being installed to the above dimensions."]
[{"$nulls":4},"The meter module offered is a single stream supply with only a nominal bypass facility.  The bypass is only used during maintenance, and is only sized to maintain gas pressure downstream. Please note that during maintenance it will be necessary to disrupt supplies. "]
[null,"All Jobs","Meter Installation with Booster","Special Features/Terms/Conditions: ","It will be necessary for the end-user to ensure that a non-return valve is installed upstream of any booster or compressor that may be installed to protect the meter installation from back pressure in the event of failure of the booster or compressor."]
[null,"All Jobs","Meter Installation with Bypass   (Twin Stream) for Single Stream change the words","Special Features/Terms/Conditions: ","The meter module offered is a twin stream supply with a bypass facility.  The bypass is only used during maintenance, and is sized to maintain full gas supply downstream. Bypass installations are subject to approval by the gas transporter. We would apply for such approval on receipt of order and work could only commence if granted."]
[null,"All Jobs","Meter installation for a special site (hospital, prison, process load etc) where the request did not specify a twin-stream governor meter module","Special Features/Terms/Conditions: ","The meter module offered is a single stream supply with no bypass facility. During maintenance operations on the meter installation it may be necessary to isolate the supply temporarily. If the load that this meter will supply is critical we recommend that you request a twin-stream design with a full bypass sufficient to maintain supply at all times."]
[null,"MP and above requests only.  Do not use for LP.","Meter Installation (or an Exchange) with an elevated metering pressure, ie > 21 mbar on the outlet","Special Features/Terms/Conditions: ","The gas metering pressure requested for this site is above the level deemed to be standard so we require a warrant from the customer to ensure the safe and reliable operation of the metering equipment and their pipework and appliances.  We have to be sure that the proposed pressures are appropriate for all of the pipework and appliances connected to the system; the information provided also dictates how the safety devices on our equipment are set up.  In order to comply with Institution of Gas Engineers Procedures we require the enclosed form GT2 to be signed and returned with your order acceptance."]
[null,"MP and IP Jobs","MP service pressure > 270 mbar\nor\nIP service pressure > 2 Bar","Special Features/Terms/Conditions: ","You will need to contact your gas transporter to arrange for an \"ancillary pressure agreement\" to ensure that the inlet pressure does not fall below the minimum service pressure of nnn mbar required for delivery of nnn mbar metering pressure.This must be supplied with the acceptance form before the order can be accepted"]
[null,"All Jobs","Meter Exchange (LP & MP)","Special Features/Terms/Conditions: ","This quotation is based on the exchange being completed on the same day and the new meter module being attached to the existing Emergency Control Valve (ECV)"]
[null,"All Jobs","2 Visit Meter Exchange\n(LP & MP)","Special Features/Terms/Conditions ","Please note that this quotation is based on two visits, first visit for the removal and purging of the existing meter module and the second to install a new meter module after the service upgrade."]
[]
["Cancellations","LP Jobs","Request for metering pressure greater than 21mb for an LP service","Special Features/Terms/Conditions","The Service Pressure to this site will not support the design criteria requested"]
[null,"All Jobs","The current meter is capable of suppling the requested Load","Special Features/Terms/Conditions","The Qmax specified in your quotation request is less than that of the meter currently installed at this Meter Point. \n\nIf the existing meter is capable of accurately registering the range of consumption required at the site it will be considered 'fit for purpose' and will therefore not be replaced. Where a meter is considered 'fit for purpose', but the customer can demonstrate that 2% of the annual gas load (AQ) flows through the meter at less than the meter's official Qmin, the meter could be considered for replacement and downsizing."]
[]
["EMS & AMR","All Jobs","EMS connection to existing meter","Special Features/Terms/Conditions: ","This quotation is based on there being a working LF connection on the existing meter"]
[null,"All Jobs","AMR with new meter","Special Features/Terms/Conditions: ","Please note the installation and connection of the AMR device is non chargeable and will be installed at a future date"]
[null,"All Jobs","All EMS connection requests\n(do not use if Housing has been requested in quotation)","Special Features/Terms/Conditions: ","Electrical Connections to gas meters are subject to the assessment of the hazardous area around the meter, this is largely affected by the ventilation in the housing, should the ventilation be found to be inadequate the connection will not be made and the requirements to allow the connection reported to you. This quotation does not include for the provision of a separate instrumentation cabinet."]
[]
["GT1","MP and above","GT1 Passed","Special Features/Terms/Conditions: ","This Quotation is based on the Medium Pressure Tier of nnn mbar,"]
[null,"MP and above","(GT1 Failures) Prior to Quoting","Special Features/Terms/Conditions: ","This Quotation is based on the Medium Pressure Tier of nnn mbar, however we believe the pressure tier to be MPnnn. Please verify the pressure tier with the Gas Transportor prior to acceptance."]
[null,"MP and above","GT1 - where the GT1 has not returned","Special Features/Terms/Conditions: ","This quote is based on a medium pressure tier of nnn mbars and is only suitable for this pressure tier.  Please verify the pressure tier with the Gas Transporter prior to acceptance to confirm suitability of the design."]
[]
["Budget Quotes","All Jobs",null,"Page 2 title","Replace the title \"Quotation\" with \"Budget Quotation\"."]
[null,"All Jobs","NGM can only provide a budget quotation","Special Features/Terms/Conditions: \n\nPlace at the top of all other caveats","National Grid Metering can only provide a budget quote from the details provided on the request form. As such, this budget quotation is based on indicative costs and dimensions only. If you require the works to proceed then National Grid Metering will require a new quotation request so that a firm quotation can be produced. Please note that this budget quotation cannot be accepted."]
[null,"All Jobs","All Jobs\nA Budget quote has been requested by the supplier","Special Features/Terms/Conditions: \n\nPlace at the top of all other caveats","As requested National Grid Metering has provided a budget quotation from the details provided on the request form.  As such, this budget quotation is based on indicative costs and dimensions only. If you require the works to proceed then National Grid Metering will require a new quotation request so that a firm quotation can be produced. Please note that this budget quotation cannot be accepted."]
[null,"IP Jobs","IP Requests Only\nGT1 can not be raised and this information can not be obtained from the Supplier.","Special Features/Terms/Conditions: ","To enable an accurate quotation, the lowest inlet pressure on an intermediate pressure service is required which can be obtained form the utility infrastructure provider (UIP) or Network.  Please confirm the inlet pressure prior to acceptance to confirm suitability of the design and the quotation provided.\n"]
[null,"All Jobs","All","Special Features/Terms/Conditions: ","Please note that full details of the design will be given once a firm quotation has been requested."]
[null,"MP and above requests only.  Do not use for LP.","Meter Installation (or an Exchange) with an elevated metering pressure, ie > 21 mbar on the outlet","Special Features/Terms/Conditions: ","The gas metering pressure requested for this site is above the level deemed to be standard. This means that a GT2 warrant will be required from the customer before any firm quotation is accepted. The warrant is to ensure the safe and reliable operation of the metering equipment and their pipework and appliances. We have to be sure that the proposed pressures will be are appropriate for all of the pipework and appliances connected to the system; the information provided will also dictates how the safety devices on our equipment are set up. "]
[null,"All Jobs","All","RAINBOW SAP\nIW52 and ME47","Delete using \"Budget Quotation\" as the reason."]